Enable

Conf t

Hostname SW1.1

Enable secret cisco

Line console 0

Password rc

Login

Exit

Service password-encryption

banner motd #\*\*\*Unauthorized access to this device is prohibited!\*\*\*#

ip domain-name cisco.com

crypto key generate rsa

:1024

username admin password rc

line vty 0 15

transport input ssh

login local

exit

vlan 10

name desenvolvimento

exit

vlan 20

name administracao

exit

vlan 30

name commercial

exit

vlan 40

name recepcao

exit

vlan 50

name area-financeira

exit

vlan 60

name reunioes

exit

vlan 70

name guest

exit

vlan 80

name perifericos

exit

vlan 90

name VOIP

exit

vlan 99

name gestao

exit

interface range F0/4 - 5

switchport mode access

switchport access vlan 10

exit

interface range F0/6 - 7

switchport mode access

switchport access vlan 20

exit

interface range F0/8 - 9

switchport mode access

switchport access vlan 30

exit

interface range F0/10 - 11

switchport mode access

switchport access vlan 40

exit

interface range F0/12 - 13

switchport mode access

switchport access vlan 50

exit

interface range F0/14 - 15

switchport mode access

switchport access vlan 60

exit

interface F0/16

switchport mode access

switchport access vlan 70

exit

interface F0/17

switchport mode access

switchport access vlan 80

exit

interface F0/18

switchport mode access

switchport voice vlan 90

exit

interface F0/19

switchport mode access

switchport access vlan 99

exit

interface vlan 99

ip address 172.20.35.130 255.255.255.240

no shutdown

exit

ip default-gateway 172.20.35.129

exit

interface f0/1

switchport mode trunk

exit